Startup GDB initialization commands for initial RAM ECC

CM4
restore ../../../../utilities/data/64KiB_0x55.bin binary 0x20000000 

N310F
restore ../../../../utilities/data/96KiB_0x55.bin binary 0x20020000 

CM7
restore ../../../../utilities/data/64KiB_0x55.bin binary 0x00000000 
restore ../../../../utilities/data/64KiB_0x55.bin binary 0x20000000
restore ../../../../utilities/data/256KiB_0x55.bin binary 0x20800000 
restore ../../../../utilities/data/128KiB_0x55.bin binary 0x20840000  
restore ../../../../utilities/data/256KiB_0x55.bin binary 0x20A00000 
restore ../../../../utilities/data/128KiB_0x55.bin binary 0x20A40000 

NX900F
restore ../../../../utilities/data/128KiB_0x55.bin binary 0x00400000 
restore ../../../../utilities/data/128KiB_0x55.bin binary 0x20480000 
restore ../../../../utilities/data/256KiB_0x55.bin binary 0x20C00000  